hAMMER MILL A/17 – R/17

[PERUZZO](https://www.peruzzo.it/en/) / [ZOO TECH](https://www.peruzzo.it/en/zoo-tech/) / HAMMER MILL A/17 – R/17

## **HAMMER MILL FOR FLOUR PRODUCTION FROM 100 TO 500 KG/HOUR.**

Hammer Mill PERUZZO mod. A/17 R/17 for grinding various cereals and cobs, for small and medium-sized farms.

PERUZZO A/17 R/17 hammer mills are available with a single-phase flanged electric motor.

The PERUZZO A/17 R/17 hammer mills have a sturdy hammer unit of which each hammer has a thickness of 8mm which facilitates the breaking of the grain immediately, producing a less gleaned flour and therefore more digestible.

The great thickness of the hammers helps the flour to be expelled through the perforated screen quickly, without altering its temperature, maintaining a high hourly production.

In addition, the PERUZZO hammers are hardened, interchangeable 4 times, guaranteeing great savings for the user.

PERUZZO hammer mills are supplied with "CE" accident prevention protections and entirely produced with Italian materials and engines.

Available perforated screens: 0.6-0.8-1-1.5-2-3-4-6-8-10-12-15-20-30