HAMMER MILL C/17-R/17

[PERUZZO](https://www.peruzzo.it/en/) / [ZOO TECH](https://www.peruzzo.it/en/zoo-tech/) / HAMMER MILL C/17-R/17

## **HAMMER MILL FOR FLOUR PRODUCTION FROM 300 TO 1300 KG/HOUR.**

The Hammer Mills PERUZZO mod. C/17 R/17 are suitable for grinding various cereals and cobs, for small and medium-sized farms.

The PERUZZO C/17 R/17 hammer mills can be supplied for PTO drive on the tractor or with electric motors.

The PERUZZO C/17 R/17 hammer mills have a sturdy hammer unit of which each hammer has a thickness of 8mm which facilitates the breaking of the wax immediately, producing a less angular flour and therefore more digestible.

The great thickness of the hammers helps the flour to be expelled through the perforated screen quickly, without altering its temperature, maintaining a high hourly production.

In addition, the hardened hammers are interchangeable 4 times, ensuring great savings for the user.

The mills are supplied with "CE" accident prevention protections and entirely produced with Italian materials and engines.

Available perforated screens: 0.6-0.8-1-1.5-2-3-4-6-8-10-12-15-20-30