HYDRAULIC ROTARY MOWER MOD. – ROTO HYDRO – PTO – BULL

[PERUZZO](https://www.peruzzo.it/en/) / [GREEN PRO](https://www.peruzzo.it/en/green-pro/) / HYDRAULIC ROTARY MOWER MOD. – ROTO HYDRO – PTO – BULL

## **КОСИЛКА ДЛЯ ГАЗОНОВ И ВЕТОК ДЛЯ ТРАКТОРОВ ОТ 30 Л.С. ДО 100 Л.С.**

**The hydraulic rotary mower mod. ROTO BULL** - mounts an oil tank and a hydraulic engine plus a blade disk that is manufactured according to CE norms for the underfoliage cutting on road or photovoltaic systems. The blades of the disc have a return-plate system that prevents the blades from touching the ground. In case of cutting around the base of small plants, the return system of the mower is regulated by springs. The cutting height is easily adjustable from 3 to 10 cm.

It is available in different versions depending on the use required:

**ROTO HYDRO**: specially designed for loaders with power between 40 and 65 liters/min., available with special connection on request for different types of wheel loaders and equipped with anti-shock and anti-avitation valve system with free-wheel, in order to prevent a damage during sudden increases of pressure inside the hydraulic engine. The Roto-Hydro coupled with a Loader is a compact equipment ideal for the maintenance of the grass along the roads as it is not cumbersome and easily manoeuvertable.

**ROTO PTO**: equipped with oil tank and hydraulic engine. It is ideal in presence of tractors of minimum 18 hp. The Roto PTO can be applied to the 3-point coupling of the tractor and has an autonomous oil pump. In this way the **ROTO** **PTO**can be moved sideways to easily reach difficult cutting areas as under canopy in orchards or solar panels.

**ROTO BULL**: hydraulic mower with independent hydraulic system and suitable for the shredder Peruzzo Mod. **BULL**.