# Spading machine

#### **150.150 SERIES**

**THEY ARE EQUIPPED WITH AN ANTI-CLOGGING FRAME WITH A DIFFERENTIATED STRUCTURE. The exclusive three-point hitch with variable distance allows you to position the spading machine closer to the tractor: easier manoeuvres - less effort for lifting, more safety and especially in the most critical conditions. MIN/MAX DEPTH 10/35 CM**

**STANDARD EQUIPMENT:**

* THREE-POINT HITCH WITH VARIABLE DISTANCE CAT II
* PROTECTED PTO SHAFT WITH CLUTCH
* DEPTH ADJUSTMENT SLIDES 18 cm
* 3-SPEED LEVER GEAR SHIFT (M9.5 HELICOIDAL) **PdF 540 = I 147 II 167 III 204** or **PdF** **1000= I 140 II 163 III 206**
* GREASE LUBRICATED ROLLER BEARINGS
* ADJUSTABLE SPUR HOOD/LEVELER
* ADJUSTABLE LEVELER

**FREE VARIABLES**

* ADJUSTABLE SPUR HOOD/LEVELER

#### **ACCESSORIES**

## **ACCESSORIES**

* **REMOVABLE LEVELER h 30 FOR SPERON COFANO.**
* **HYDRAULIC ADJUSTMENT FOR SPUR HOOD**
* **POSTERIOR EXIT PdF13/8Z6**
* **LUBRICATION OF CONNECTING RODS WITH STEEL SEALS**
* **DOUBLE TOP HOOD**
* **LEVELER EXTENSION**
* **LATERAL SPILLWAYS**
* **LONG SPADES FOR SANDY SOILS**
* **ROUND SPADES FOR SOILS WITH STONES**
* **WIDE SPADES FOR PADDY/KIWI FIELDS**
* **2 FOREQUARTERS**H15/45 cm 6/18 inc.
* **SLIDES WIDTH** 40 cm
* **REAR THREE-POINT ATTACHMENT**+kg 150/Lbs 331 – cat II
* **SUPPORT WHEELS**(see below)

