**Find Top-Quality Trailer Mounted Tree Spades for Efficient Landscaping**

Big John’s trailer-mounted tree spades are your solution for efficient and reliable tree transplanting. Designed for ease of transport and exceptional durability, our spades help you elevate your farming and landscaping projects to the next level.

Experience the difference that quality equipment can make. Contact us today to discuss your needs and get the best trailer-mounted tree spades on the market!

**44DTG**

1 – 10 cm Trees

Compact and Sturdy

The 44DTG is one of the smaller trailer spades that operates with simplicity and durability. Made with AR400 spade material, the Model 44 is made for trailers 449 cm in length and comes with hydraulic rear stabilizers and an extendable trailer tongue.

| **44DTG SPECS** |  |
| --- | --- |
| Trailer Length | 449 cm |
| Trailer Width | 250 |
| Tree Trunk Diameter | 1 – 10 cm |
| Root Ball Width | 111 cm |
| Root Ball Depth | 91 cm |
| Root Ball Weight (approx.) | 612 kg |
| Machine Weight (empty/loaded) | 2490/3100 kg |
| Transport Height | 305 cm |
| Blade Tower Height (down position) | 210 cm |
| Gate Opening | 60 cm |
| Opening Width | 225 cm |
| Number of Spades | 4 |
| Hydraulic Gate Lock | Yes |
| Spade Material | AR400 |
| Drive System (minimum GPM) | 14 |
| Hydraulic Tongue Ext | Yes |
| Tongue Swivel Left/Right | 30°/30° |
| Hydraulic Jack Stand | Yes |
| Adjust. Hydraulic Pads | No |
| Adjust. Mechanical Pads | No |

**54**

1 – 10 cm Trees

Adaptable and Functional

The 54 Trailer Spade features our newest trailer design. It is a versatile trailer that comes in various sizes to fit any BIG JOHN customer's needs.

The 54 Trailer Spade comes with an extendable trailer tongue, hydraulic jack, and hydraulic rear stabilizers. It also comes available in single axle 42 and 44" trailers. Our new design offers the same durable and reliable features as the rest of our BIG JOHN trailer lineup.

| **MODEL 54 SPECS** |  |
| --- | --- |
| Nominal Tree Trunk Diameter | 1 – 10 cm |
| Root Ball Width | 111 cm |
| Root Ball Depth | 91 cm |
| Root Ball Weight | 544 kg |
| Total Machine Weight | 952 kg |
| Blade Tower Height | 210 cm |
| Gate Opening | 60 cm |
| Opening Width | 243 cm |
| Number of Spades | 4 |
| Hydraulic Gate Lock | Yes |
| Adjustable Hydraulic Pads | Yes |
| Adjustable Mechanical Pads | Yes |
| Spade Material | AR400 |
| Drive System (Minimum GPM) | 10 – 16 GPM / 37 – 60 LPM |

**55DTD**

10 – 12,5 cm Trees

Durable and Versatile

The model 55DTD is part of the Trailer Mounted family that comes with the same durability and reliability as the rest. It can handle trees up to 12,5 cm in diameter, comes with a hydraulic lock and tongue, and is made with AR500 spade material.

| **55DTD SPECS** |  |
| --- | --- |
| Trailer Length | 599 cm |
| Trailer Width | 243 cm |
| Tree Trunk Diameter | 10 – 12,5 cm |
| Root Ball Width | 132 cm |
| Root Ball Depth | 121 cm |
| Root Ball Weight (approx.) | 1630 kg |
| Total Machine Weight | 4762 kg |
| Transport Height | 335 cm |
| Blade Tower Height (down position) | 200 cm |
| Gate Opening | 76 cm |

**65DTD**

15 – 17,5 cm Trees

Durable and Reliable

The 65DTD is another standard Trailer Mounted spade that comes with the same quality as the rest. The Model 65DTD can handle trees up to 17,5 cm in diameter and is made with AR500 spade material. It comes with a hydraulic lock and tongue.

| **65DTD SPECS** |  |
| --- | --- |
| Trailer Length | 599 cm |
| Trailer Width | 243 cm |
| Tree Trunk Diameter | 15 – 17,5 cm |
| Root Ball Width | 157 cm |
| Root Ball Depth | 134 cm |
| Root Ball Weight (approx.) | 1950 kg |
| Total Machine Weight | 4985 kg |
| Transport Height | 353 cm |
| Blade Tower Height (down position) | 218 cm |
| Gate Opening | 101 cm |