**WALK BEHIND SAND CLEANER:**

**THE BARBER SAND MAN™ 850**

The BARBER SAND MAN 850 is a compact, self-propelled, and walk behind sand cleaner that offers dependability and maneuverability and is an effective sand cleaner for removing debris from virtually **any small sandy area, regardless of location and space restrictions.**

**SAND SIFTING AND SOIL SCREENING APPLICATIONS**

The SAND MAN 850 is a versatile sand sifter and soil screener that has a wide variety of applications. Its maneuverability, effectiveness, and ease of operation make it a valuable tool for golf course owners, small beach owners, and anyone who maintains smaller sandy areas. By screening stones, litter, shells, glass, and other finer objects, the SAND MAN ensures your property will be debris-free. Learn more about how the SAND MAN is effective for the featured applications:

Beaches

Golf Bunkers

Infield Cleaning

Volleyball Courts, Cabanas

Oil Spill Beach Cleanup

**FEATURES:**

The SAND MAN is a light- weight, easily maneuverable, walk behind sand sifter. The sieving unit is compact enough to be transported in the bed of a pickup truck and lightweight enough to be unloaded by one person.

**easy maneuverability**

Independent brakes on each wheel and a differential lock, which assists in soft sand conditions, aid maneuverability.

**reliable components**

The walk behind sand sifter is propelled by high flotation rubber tires, which provide excellent traction in sand but will not harm grass or paved surfaces. The SAND MAN is powered by a reliable, noise restricted, 5.5HP HONDA gasoline engine.

**sift a variety of materials**

The SAND MAN sand sifter elevates the sand and utilizes a sifting screen to sieve the debris. The debris is then deposited into the collector. There are three interchangeable screens with mesh sizes of 3/16″, 3/8″ & 1/2″. Different sieve size is determined by the application. The sand sifter’s smaller mesh is used for ultra fine cleaning and the larger mesh allows for deeper cleaning and rapid sifting speed in wet sand.

**adjustable cleaning depth**

The operator, while the machine is in use, can easily adjust the cleaning depth, from 0-4″.

**high capacity & easy transport**

The 5.3 gallon (20 liter) collector can be easily emptied into either of the on-board storage hoppers for a total capacity of 14 gallons (54 liters). The self-propelled machine makes transporting debris to disposal sights painless.